1. 
make sure you installed all drivers from NTool drivers folder
2. 
unpack P2C_BootFix.zip into some folder, like c:\bootfix, open command prompt and go to this folder
3. 
disassemble phone ( preheat display or you will surely damage it )
4. 
connect marked testpoint to +3.3v source, battery "+" connector will do job just fine
5. 
connect phone to PC, if you do job well, then you will see "Qualcomm HS-USB QDLoader 9008" port, not ADB Fastboot port
6. 
immediately run load_fh.cmd and check if loader uploaded okay, if not - disconnect cable, reconnect battery and proceed from p.4
7. 
run load_boot.cmd
8. 
your phone is ready to be flashed with whatever firmware you want

