############################################################################################################
#
#  General Setting
#
############################################################################################################
- general: MTK_PLATFORM_CFG
  info: 
    - config_version: V1.1.2
      platform: MT6737M
      project: NE1
      storage: EMMC
      boot_channel: MSDC_0
      block_size: 0x20000
############################################################################################################
#
#  Layout Setting
#
############################################################################################################
- partition_index: SYS0
  partition_name: preloader
  file_name: NE1-0-215O-preloader_NE1.bin
  is_download: false
  type: SV5_BL_BIN
  linear_start_addr: 0x0
  physical_start_addr: 0x0
  partition_size: 0x40000
  region: EMMC_BOOT_1
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: BOOTLOADERS
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS1
  partition_name: pgpt
  file_name: NONE
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x0
  physical_start_addr: 0x0
  partition_size: 0x80000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: INVISIBLE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS2
  partition_name: proinfo
  file_name: NONE
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x80000
  physical_start_addr: 0x80000
  partition_size: 0x300000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: PROTECTED
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS3
  partition_name: nvram
  file_name: NONE
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x380000
  physical_start_addr: 0x380000
  partition_size: 0x500000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: BINREGION
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS4
  partition_name: protect1
  file_name: NONE
  is_download: false
  type: EXT4_IMG
  linear_start_addr: 0x880000
  physical_start_addr: 0x880000
  partition_size: 0xa00000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: PROTECTED
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS5
  partition_name: protect2
  file_name: NONE
  is_download: false
  type: EXT4_IMG
  linear_start_addr: 0x1280000
  physical_start_addr: 0x1280000
  partition_size: 0xa00000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: PROTECTED
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS6
  partition_name: lk
  file_name: NE1-0-215O-lk.bin
  is_download: true
  type: NORMAL_ROM
  linear_start_addr: 0x1c80000
  physical_start_addr: 0x1c80000
  partition_size: 0x80000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: true
  reserve: 0x00

- partition_index: SYS7
  partition_name: para
  file_name: NONE
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x1d00000
  physical_start_addr: 0x1d00000
  partition_size: 0x80000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: INVISIBLE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS8
  partition_name: boot
  file_name: NE1-0-215O-00WW-boot.img
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x1d80000
  physical_start_addr: 0x1d80000
  partition_size: 0x1000000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS9
  partition_name: recovery
  file_name: NE1-0-215O-00WW-recovery.img
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x2d80000
  physical_start_addr: 0x2d80000
  partition_size: 0x1000000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS10
  partition_name: logo
  file_name: NE1-0-215O-logo.bin
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x3d80000
  physical_start_addr: 0x3d80000
  partition_size: 0x800000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: true
  reserve: 0x00

- partition_index: SYS11
  partition_name: expdb
  file_name: NONE
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x4580000
  physical_start_addr: 0x4580000
  partition_size: 0xa00000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: INVISIBLE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS12
  partition_name: seccfg
  file_name: NONE
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x4f80000
  physical_start_addr: 0x4f80000
  partition_size: 0x80000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: INVISIBLE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS13
  partition_name: oemkeystore
  file_name: NONE
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x5000000
  physical_start_addr: 0x5000000
  partition_size: 0x200000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: INVISIBLE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS14
  partition_name: secro
  file_name: NE1-0-215O-secro.img
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x5200000
  physical_start_addr: 0x5200000
  partition_size: 0x600000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS15
  partition_name: keystore
  file_name: NONE
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x5800000
  physical_start_addr: 0x5800000
  partition_size: 0x800000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: INVISIBLE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS16
  partition_name: tee1
  file_name: NE1-0-215O-trustzone.bin
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x6000000
  physical_start_addr: 0x6000000
  partition_size: 0x500000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: true
  reserve: 0x00

- partition_index: SYS17
  partition_name: tee2
  file_name: NE1-0-215O-trustzone.bin
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x6500000
  physical_start_addr: 0x6500000
  partition_size: 0x500000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS18
  partition_name: box
  file_name: NONE
  is_download: false
  type: EXT4_IMG
  linear_start_addr: 0x6a00000
  physical_start_addr: 0x6a00000
  partition_size: 0x800000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: INVISIBLE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS19
  partition_name: sys_info
  file_name: fver
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x7200000
  physical_start_addr: 0x7200000
  partition_size: 0x100000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS20
  partition_name: sutinfo
  file_name: NE1-00WW-001-sutinfo.img
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x7300000
  physical_start_addr: 0x7300000
  partition_size: 0x20000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS21
  partition_name: hidden
  file_name: -hidden.img.ext4
  is_download: false
  type: EXT4_IMG
  linear_start_addr: 0x7320000
  physical_start_addr: 0x7320000
  partition_size: 0x2000000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS22
  partition_name: cda
  file_name: NE1-00WW-010-cda.img
  is_download: false
  type: EXT4_IMG
  linear_start_addr: 0x9320000
  physical_start_addr: 0x9320000
  partition_size: 0x800000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS23
  partition_name: frp
  file_name: NONE
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0x9b20000
  physical_start_addr: 0x9b20000
  partition_size: 0x100000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: INVISIBLE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS24
  partition_name: nvdata
  file_name: NONE
  is_download: false
  type: EXT4_IMG
  linear_start_addr: 0x9c20000
  physical_start_addr: 0x9c20000
  partition_size: 0x2000000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: INVISIBLE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS25
  partition_name: metadata
  file_name: NONE
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0xbc20000
  physical_start_addr: 0xbc20000
  partition_size: 0x23e0000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: INVISIBLE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS26
  partition_name: system
  file_name: NE1-0-215O-00WW-system.img
  is_download: false
  type: EXT4_IMG
  linear_start_addr: 0xe000000
  physical_start_addr: 0xe000000
  partition_size: 0x100000000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS27
  partition_name: cache
  file_name: cache.img
  is_download: false
  type: EXT4_IMG
  linear_start_addr: 0x10e000000
  physical_start_addr: 0x10e000000
  partition_size: 0x19000000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS28
  partition_name: userdata
  file_name: userdata.img
  is_download: false
  type: EXT4_IMG
  linear_start_addr: 0x127000000
  physical_start_addr: 0x127000000
  partition_size: 0x60000000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: true
  is_reserved: false
  operation_type: UPDATE
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS29
  partition_name: flashinfo
  file_name: NONE
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0xFFFF0084
  physical_start_addr: 0xFFFF0084
  partition_size: 0x1000000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: false
  is_reserved: true
  operation_type: RESERVED
  empty_boot_needed: false
  reserve: 0x00

- partition_index: SYS30
  partition_name: sgpt
  file_name: NONE
  is_download: false
  type: NORMAL_ROM
  linear_start_addr: 0xFFFF0004
  physical_start_addr: 0xFFFF0004
  partition_size: 0x80000
  region: EMMC_USER
  storage: HW_STORAGE_EMMC
  boundary_check: false
  is_reserved: true
  operation_type: RESERVED
  empty_boot_needed: false
  reserve: 0x00

